## Information

# EyePoint S

Autonomous two-channel desktop localizer of faulty electronic components on printed circuit boards using the analog signature analysis method with a test signal frequency of up to 100 kHz. The system has a large, user-friendly touch screen. An additional pedal allows for easier control of the system. The device has a test plan mode, which allows you to save a reference board in advance and then work with the same faulty board without having a reference at hand.